| Visioscan Set SDK Libraries 1.3.5 Visioscan Set SDK Help documentation file for C++ and C++/CLI |

Loading...
Searching...
No Matches
Introduction

This project intends to ensure sensor's encapsulation.

# Getting Started

## 1. Installation process

The prerequisists LIBUSB must be checked out prior to build any project. Solution structure must be:

-- Working Directory
|
-- Solution Folder (the place I will checkout this solution)
|
-- libusb-source (the place I will checkout the libusb source code)
|
-- android
|
-- build
|
-- doc
|
-- (...)
|
-- libusb (<- libusb sources)

## 2. Software dependencies

Solution depends on the libusb source code (which can be fount here https://github.com/libusb/libusb.git) To ensure that dependencies are well distributed, OUTPUT directories must be set to the same Solution projects output directory. Otherwise, compile and link may fail.

## 3. Latest releases

Master is the latest release

## 4. API references

API documentation can be generated using DOxygen tool

# Requirements, Build and Test

Windows SDK Version: 10.0
Platform toolset: Visual Studio 2022 (v143)
C++ Language Standard: ISO C++ 14 Standard.
Open visual studio 2022, build the solution in any variant you want