| Visioscan Set SDK Libraries 1.3.5 Visioscan Set SDK Help documentation file for C++ and C++/CLI |

Loading...
Searching...
No Matches
AgvSensor Member List

This is the complete list of members for AgvSensor, including all inherited members.

AbortLearning() | AgvSensor |
AgvSensor() | AgvSensor |
AgvSensor(BaseCommunication *comm) | AgvSensor |
Close() | AgvSensor |
GetAbortStatus() | AgvSensor |
GetAngleRange() | AgvSensor |
GetContaminationStatus() | AgvSensor |
GetContaminationThreshold() | AgvSensor |
GetDataPacketType() | AgvSensor |
GetDefaultValues() | AgvSensor |
GetDeviceName() | AgvSensor |
GetErrorLog() | AgvSensor |
GetField(uint8_t fieldNumber, NativeZoneTypeEnum zone) | AgvSensor |
GetFieldName(int fieldSetNumber) | AgvSensor |
GetImmunityLevel() | AgvSensor |
GetInputControlModeStatus() | AgvSensor |
GetInputStatus() | AgvSensor |
GetLearningErrorCode() | AgvSensor |
GetLearningStatus() | AgvSensor |
GetNetworkInformation() | AgvSensor |
GetObjectSize() | AgvSensor |
GetOffDelay() | AgvSensor |
GetOnDelay() | AgvSensor |
GetOutputActiveLevel() | AgvSensor |
GetOutputFunction() | AgvSensor |
GetOutputStatus() | AgvSensor |
GetPlatformVersion() | AgvSensor |
GetRawDataExchangeMode() | AgvSensor |
GetRuntimeHours() | AgvSensor |
GetSelectedField() | AgvSensor |
GetSensorLamps() | AgvSensor |
GetSensorLeds() | AgvSensor |
GetTemperature() | AgvSensor |
GetUncoverZoneSize() | AgvSensor |
GetVersion() | AgvSensor |
GetWarningSpot() | AgvSensor |
GetWms() | AgvSensor |
GetZone1Mode() | AgvSensor |
Initialize() | AgvSensor |
RebootDevice() | AgvSensor |
RequestChallenge() | AgvSensor |
ResetAllFields() | AgvSensor |
ResetDevice() | AgvSensor |
RetrieveRawData() | AgvSensor |
SendCypher(string cypher) | AgvSensor |
SendMdi() | AgvSensor |
SetAngleRange(AngleRange pAngleRange) | AgvSensor |
SetContaminationThreshold(ContaminationThreshold pContaminationThreshold) | AgvSensor |
SetDataPacketType(SCAN_PACKET_TYPE pPacketType) | AgvSensor |
SetDeviceName(string pName) | AgvSensor |
SetField(FieldData data) | AgvSensor |
SetFieldName(FieldName fieldName) | AgvSensor |
SetHoldTime(HoldTime holdTime) | AgvSensor |
SetImmunityLevel(int pImmunityLevel) | AgvSensor |
SetInputControlModeStatus(NativeInputControleModeStatus controlMode) | AgvSensor |
SetInputsValue(NativeActiveLevelEnum input1, NativeActiveLevelEnum input2, NativeActiveLevelEnum input3, NativeActiveLevelEnum input4) | AgvSensor |
SetMultipleSampling(MultipleSampling sampling) | AgvSensor |
SetNetworkInformation(NetworkInformation pNetwork) | AgvSensor |
SetObjectSize(ObjectSize sizeToSet) | AgvSensor |
SetOffDelay(OnOffDelay offDelay) | AgvSensor |
SetOnDelay(OnOffDelay onDelay) | AgvSensor |
SetOutputActiveLevel(ActiveLevel activeLevel) | AgvSensor |
SetOutputFunction(OutputFunction function) | AgvSensor |
SetRawDataExchangeMode(PROTOCOL pProtocol) | AgvSensor |
SetSensorLeds(AgvSensorLeds leds) | AgvSensor |
SetUncoverZoneSize(UncoverZone uncoverZoneToSet) | AgvSensor |
SetWarningSpot(WarningSpot spotToSet) | AgvSensor |
SetZone1Mode(NativeZoneModeEnum mode) | AgvSensor |
StartLearning(uint8_t fieldNumber, NativeZoneTypeEnum zone, uint16_t uncover, NativeObjSizeEnum objectSize) | AgvSensor |
StopLearning() | AgvSensor |
StopMdi() | AgvSensor |
StoreInFlash() | AgvSensor |
~AgvSensor() | AgvSensor |