| Visioscan Set SDK Libraries 1.3.5 Visioscan Set SDK Help documentation file for C++ and C++/CLI |

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - s -

- semReadyToConsume : UsbDevice
- SendCommand() : abstract, EthernetCommunication, UsbCommunication
- SendCypher() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SendMDI : abstract
- SendMdi() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, RawDataSensor, WRawDataSensor
- SensorErrorException() : SensorErrorException
- SensorLamps() : SensorLamps
- SensorLeds() : SensorLeds
- SetAddress() : DevicePinger
- SetAngleRange() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues, RawDataSensor, WRawDataSensor
- SetAngularResolution() : NavigationSensor, RawDataSensor, WNavigationSensor, WRawDataSensor
- SetBusNumber() : UsbInformation
- SetCanNumber() : SoftwareVersion
- SetCode() : AvailableResolution
- SetCommunication() : abstract
- SetCommunicationCallback() : abstract
- SetCont : abstract
- SetContaminationLed() : AgvSensorLeds
- SetContaminationThreshold() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues, RawDataSensor, WRawDataSensor
- SetCrc() : FieldData
- SetCurrentFramePosition() : abstract
- SetData() : FieldData
- SetDataExtractor() : abstract
- SetDataLeft() : ContaminationStatus
- SetDataMiddle() : ContaminationStatus
- SetDataPacketType() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, RawDataSensor, WRawDataSensor
- SetDataRecorder() : abstract
- SetDataRight() : ContaminationStatus
- SetDeviceAddress() : UsbInformation
- SetDeviceName() : abstract, AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues, RawDataSensor, WBase::abstract, WRawDataSensor
- SetDHCP : abstract
- SetDhcpMode() : NetworkInformation
- SetDir : abstract
- SetDisplayMode() : NavigationSensor, WNavigationSensor
- SetDisplayPageDirection() : NavigationSensor, WNavigationSensor
- SetDisplayPageIndex() : NavigationSensor, WNavigationSensor
- SetDisplayWakeUpRange() : NavigationSensor, WNavigationSensor
- SetDisplayWakeUpTime() : NavigationSensor, WNavigationSensor
- SetError() : ContaminationThreshold
- SetErrorCode() : RawDataError
- SetErrorDate() : RawDataError
- SetErrorLevel() : ActiveLevel
- SetEthCfg : abstract
- SetFar() : HoldTime, MultipleSampling, ObjectSize, OnOffDelay, UncoverZone, WarningSpot
- SetFarZoneName() : FieldName
- SetField() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetFieldName() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetFieldNumber() : FieldData, FieldName
- SetFilter : abstract
- SetFilterMode() : FilterType
- SetFilterStatus() : RawDataSensor, WRawDataSensor
- SetFilterType() : NavigationSensor, WNavigationSensor
- SetFrameRate() : abstract
- SetGateway() : NetworkInformation
- SetGUID() : FieldData
- SetGW : abstract
- SetHardwareVersion() : SoftwareVersion
- SetHoldTime() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetImmu : RawDataSensor
- SetImmunityLevel() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, NavigationSensor, RawDataSensor, WRawDataSensor
- SetInputControlModeStatus() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetInputsValue() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetIP : abstract
- SetIp() : EthernetSettings
- SetIpAddress() : NetworkInformation
- SetIpPort() : NetworkInformation
- SetLED : abstract
- SetLed1() : SensorLamps
- SetLed2() : SensorLamps
- SetLed3() : SensorLamps
- SetLed4() : SensorLamps
- SetLevel1() : ActiveLevel
- SetLevel2() : ActiveLevel
- SetLevel3() : ActiveLevel
- SetLevel4() : ActiveLevel
- SetLogoImage() : NavigationSensor, WNavigationSensor
- SetLogoLed() : SensorLeds
- SetMacAddress() : NetworkInformation
- SetMainName() : FieldName
- SetManufacturer() : UsbInformation
- SetMask : abstract
- SetMiddle() : HoldTime, MultipleSampling, ObjectSize, OnOffDelay, UncoverZone, WarningSpot
- SetMiddleZoneName() : FieldName
- SetMultipleSampling() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetName : abstract, AvailableResolution
- SetNear() : HoldTime, MultipleSampling, ObjectSize, OnOffDelay, UncoverZone, WarningSpot
- SetNearZoneName() : FieldName
- SetNetworkInformation() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, RawDataSensor, WRawDataSensor
- SetNumH() : FilterType
- SetNumS() : FilterType
- SetObjectSize() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues
- SetOffDelay() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetOffDelays() : DefaultValues
- SetOnDelay() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetOnDelays() : DefaultValues
- SetOutput1() : OutputFunction
- SetOutput2() : OutputFunction
- SetOutput3() : OutputFunction
- SetOutput4() : OutputFunction
- SetOutputActiveLevel() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues
- SetOutputFunction() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues
- SetParameter1() : FieldData
- SetParameter2() : FieldData
- SetPartNumber() : SoftwareVersion
- SetPort : abstract
- SetProductDescription() : UsbInformation
- SetProductId() : UsbInformation, UsbSettings
- SetProductIdentification() : SoftwareVersion
- SetProto : abstract
- SetPrototype() : SoftwareVersion
- SetPType : abstract
- SetRange : abstract
- SetRawDataExchangeMode() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, RawDataSensor, WRawDataSensor
- SetReadChannel() : UsbSettings
- SetResol : abstract
- SetResult() : ConfigurationResult
- SetRevision() : SoftwareVersion
- SetScanningDirection() : RawDataSensor, WRawDataSensor
- SetSensorLeds() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues, NavigationSensor, RawDataSensor, WNavigationSensor, WRawDataSensor
- SetSerialNumber() : UsbInformation
- SetSettings() : abstract
- SetSkip : abstract
- SetSkipScan() : RawDataSensor, WRawDataSensor
- SetSpeed() : UsbInformation
- SetStart() : AngleRange
- SetStatusLed() : SensorLeds
- SetStop() : AngleRange
- SetSubnetMask() : NetworkInformation
- SetTcpPort() : EthernetSettings
- Settings : WBase::abstract
- SetTotalFrame() : abstract
- SetTranslateCode() : abstract
- SetUdpPort() : EthernetSettings
- SetUncoverZoneSize() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetVendorId() : UsbInformation, UsbSettings
- SetVersion() : SoftwareVersion
- SetWarning() : ContaminationThreshold
- SetWarningSpot() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, DefaultValues
- SetWCalib : abstract
- SetWriteChannel() : UsbSettings
- SetZ1() : ContaminationStatus
- SetZ2() : ContaminationStatus
- SetZ3() : ContaminationStatus
- SetZ4() : ContaminationStatus
- SetZ5() : ContaminationStatus
- SetZ6() : ContaminationStatus
- SetZ7() : ContaminationStatus
- SetZ8() : ContaminationStatus
- SetZ9() : ContaminationStatus
- SetZone1Mode() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- SetZoneMode() : DefaultValues
- SetZoneType() : FieldData
- ShowDeviceIdentification() : NavigationSensor, WNavigationSensor
- SPC : abstract
- Split() : Utility
- src_portno : udp_hdr
- Start : WAngleRange
- StartLearning() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- StartMonitoring() : abstract
- StartWindowCalibration() : RawDataSensor
- StartWindowCalibrationStatus() : WRawDataSensor
- Status : CommunicationStatus, WBase::abstract
- StatusLed : WSensorLeds
- Stop() : abstract, FileDataRecorder, WBase::abstract, WRecorder::WFileDataRecorder
- StopLearning() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- StopMDI : abstract
- StopMdi() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor, RawDataSensor, WRawDataSensor
- StopMonitoring() : abstract
- STOPPED : abstract
- StoreInFlash() : AgvSensor, Com::AgvSensorWrapper::Sensor::WAgvSensor
- success : ping_result